|  |  |  |  |
| --- | --- | --- | --- |
| **Title:** | First Observation of Photon-Photon Resonance in Active Multimode Interferometer Laser Diode | | |
| **Author(s) Name:** | M. N. Uddin, H. Bingzhou, A. Tajima, K. Kato, and K. Hamamoto | | |
| **Contact Email(s):** | drnasir@aiub.edu | | |
| **Published Journal Name:** | Technical digest of European Conference on Integrated Optics (ECIO 17th) and the MicroOptics Conference (MOC 19th), Nice, France, 24-27 June 2014 | | |
| **Type of Publication:** | Conference | | |
| **Volume:** |  | Issue |  |
| **Publisher:** | ECIO, FRANCE | | |
| **Publication Date:** | June 2014 | | |
| **ISSN:** |  | | |
| **DOI:** | <https://www.ecio-conference.org/2014-proceedings/> | | |
| **URL:** | https://www.ecio-conference.org/wp-content/uploads/2016/05/2014/ECIO-2014\_Th4aR07.pdf | | |
| **Other Related Info.:** | Page Th4aR7 | | |
|  | | | |

|  |  |
| --- | --- |
| **Abstract:** |  |
| Active multimode interferometer laser diode (MMI-LD) with split pump section have been fabricated to achieve high 3 dB bandwidth. Higher photon density using split pump scheme and high-frequency photon-photon resonance has been exploited to extend the direct modulation bandwidth. The split pump active MMI design allows interaction between the lasing mode and a second mode used as catalyst in the pumping section to achieve PPR peak along with the higher photon density delivered by the MMI pumping section towards the modulation section, which allowed us to reach a more than 15.2 GHz of extended 3 dB bandwidth for the active MMI LD | |