|  |  |  |  |
| --- | --- | --- | --- |
| **Title:** | Transient Stability Enhancement of a Grid-Connected Large-Scale PV System Using Fuzzy Logic Controller | | |
| **Author(s) Name:** | Md. Rifat Hazari, Effat Jahan, Mohammad Abdul Mannan and Narottam Das | | |
| **Contact Email(s):** | effat@aiub.edu | | |
| **Published Journal Name:** | Electronics | | |
| **Type of Publication:** | Journal | | |
| **Volume:** | 10 | Issue | 9 |
| **Publisher:** | MDPI | | |
| **Publication Date:** | Oct. 8, 2021 | | |
| **ISSN:** | 2079-9292 | | |
| **DOI:** | https://doi.org/10.3390/electronics10192437 | | |
| **URL:** | https://www.mdpi.com/2079-9292/10/19/2437 | | |
| **Other Related Info.:** | Page 1-14 | | |
|  | | | |

|  |  |
| --- | --- |
| **Abstract:** |  |
| This paper presents a new intelligent control strategy to augment the low-voltage ride-through (LVRT) potential of photovoltaic (PV) plants, and the transient stability of a complete grid system. Modern grid codes demand that a PV plant should be connected to the main power system during network disturbance, providing voltage support. Therefore, in this paper, a novel fuzzy logic controller (FLC) using the controlled cascaded strategy is proposed for the grid side converter (GSC) of a PV plant to guarantee voltage recovery. The proposed FLC offers variable gains based upon the system requirements, which can inject a useful amount of reactive power after a severe network disturbance. Therefore, the terminal voltage dip will be low, restoring its pre-fault value and resuming its operation quickly. To make it realistic, the PV system is linked to the well-known IEEE nine bus system. Comparative analysis is shown using power system computer-aided design/electromagnetic transients including DC (PSCAD/EMTDC) software between the conventional proportional–integral (PI) controller-based cascaded strategy and the proposed control strategy to authenticate the usefulness of the proposed strategy. The comparative simulation results indicate that the transient stability and the LVRT capability of a grid-tied PV system can be augmented against severe fault using the proposed FLC-based cascaded GSC controller. | |