|  |  |  |  |
| --- | --- | --- | --- |
| **Title:** | Primary frequency control of large-scale PV-connected multi-machine power system using battery energy storage system | | |
| **Author(s) Name:** | S. M. Imrat Rahman, Md. Rifat Hazari, Sumaiya Umme Hani, Bishwajit Banik Pathik, Mohammad Abdul Mannan, Asif Mahfuz, Mohammad Khurshed Alam, and Md. Kamrul Hassan | | |
| **Contact Email(s):** | rifat@aiub.edu | | |
| **Published Journal Name:** | International Journal of Power Electronics and Drive System(IJPEDS) | | |
| **Type of Publication:** | Journal | | |
| **Volume:** | 12 | Issue | 3 |
| **Publisher:** | Institute of Advanced Engineering and Science (IAES) | | |
| **Publication Date:** | Sept. 30, 2021 | | |
| **ISSN:** | 2088-8694 | | |
| **DOI:** | http://doi.org/10.11591/ijpeds.v12.i3.pp1862-1871 | | |
| **URL:** | https://ijpeds.iaescore.com/index.php/IJPEDS/article/view/21459 | | |
| **Other Related Info.:** | Page 1862-1871 | | |
|  | | | |

|  |  |
| --- | --- |
| **Abstract:** |  |
| Large-scale grid-tied photovoltaic (PV) station are increasing rapidly. However, this large penetration of PV system creates frequency fluctuation in the grid due to the intermittency of solar irradiance. Therefore, in this paper, a robust droop control mechanism of the battery energy storage system (BESS) is developed in order to damp the frequency fluctuation of the multi-machine grid system due to variable active power injected from the PV panel. The proposed droop control strategy incorporates frequency error signal and dead-band for effective minimization of frequency fluctuation. The BESS system is used to consume/inject an effective amount of active power based upon the frequency oscillation of the grid system. The simulation analysis is carried out using PSCAD/EMTDC software to prove the effectiveness of the proposed droop control-based BESS system. The simulation result implies that the proposed scheme can efficiently curtail the frequency oscillation. | |