|  |  |  |  |
| --- | --- | --- | --- |
| Title | [Numerical solution of bio-nano-convection transport from a horizontal plate with blowing and multiple slip effects](https://journals.sagepub.com/doi/abs/10.1177/0954406219867985) | | |
| Author(s) Name | Uddin M Jashim, Muhammad N Kabir, Yasser Alginahi, O Anwar Bég | | |
| Contact Email(s) | ***jashim\_74@yahoo.com*** | | |
| Published Journal Name | Journal of Mechanical Engineering Science | | |
| Type of Publication | Journal | | |
| Volume | 233 | Issue | 19-20 |
| Publisher | SAGE | | |
| Publication Date | 2019/10 | | |
| ISSN | 0954-4062 | | |
| DOI | * [https://doi.org/10.1177/0954406219867985](https://doi.org/10.1177%2F0954406219867985) | | |
| URL |  | | |
| Other Related Info. |  | | |
|  | | | |

|  |  |
| --- | --- |
| Abstract |  |

In this paper, a new bio-nano-transport model is presented. The effects of first- and second-order velocity slips, thermal slip, mass slip, and gyro-tactic (torque-responsive) microorganism slip of bioconvective nanofluid flow from a moving plate under blowing phenomenon are numerically examined. The flow model is expressed by partial differential equations which are converted to a similar boundary value problem by similarity transformations. The boundary value problem is converted to a system of nonlinear equations which are then solved by a Matlab nonlinear equation solver *fsolve* integrated with a Matlab ODE solver *ode15s*. The effects of selected control parameters (first order slip, second order slip, thermal slip, microorganism slip, blowing, nanofluid parameters) on the non-dimensional velocity, temperature, nanoparticle volume fraction, density of motile micro-organism, skin friction coefficient, heat transfer rate, mass flux of nanoparticles and mass flux of microorganisms are analyzed. Our analysis reveals that a higher blowing parameter enhances micro-organism propulsion, flow velocity and nano-particle concentration, and increases the associated boundary layer thicknesses. A higher wall slip parameter enhances mass transfer and accelerates the flow. The MATLAB computations have been rigorously validated with the second-order accurate finite difference Nakamura tri-diagonal method. The current study is relevant to microbial fuel cell technologies which combine nanofluid transport, bioconvection phenomena and furthermore can be applied in nano-biomaterials sheet processing systems