|  |  |  |  |
| --- | --- | --- | --- |
| **Title:** | Design, Implementation and Analysis of a MAGLEV Wind Turbine | | |
| **Author(s) Name:** | Ariq Rahman Pranto, Muide Muktadir Aumio, Mujtahid Ahammad, Anik Sarker, Md. Shahariar Parvez, Abir Ahmed and Md. Rifat Hazari | | |
| **Contact Email(s):** | rifat@aiub.edu | | |
| **Published Conference Name:** | 2021 International Conference on Automation, Control and Mechatronics for Industry4.0 (ACMI) | | |
| **Type of Publication:** | International Conference | | |
| **Volume:** |  | Issue |  |
| **Publisher:** | IEEE | | |
| **Publication Date:** | Sept. 8, 2021 | | |
| **ISSN:** |  | | |
| **DOI:** | https://ieeexplore.ieee.org/document/9528131 | | |
| **URL:** | https://doi.org/10.1109/ACMI53878.2021.9528131 | | |
| **Other Related Info.:** | Pages 1-4 | | |
|  | | | |

|  |  |
| --- | --- |
| **Abstract:** |  |
| Conventionally, horizontal axis wind turbine (HAWT) is used in the wind farm applications to generate electricity. But HAWT is very expensive to install, noisy and inefficient in the conversion of wind to energy. Additionally, it requires large amount to space, high wind speed and also it is dependent upon the direction of wind speed. If direction of the wind is changed then it requires Yaw mechanism which is very expensive. On the other hand, the MAGLEV vertical axis wind turbine (VAWT) addresses these problems and provides a more efficient, versatile and elegant method of producing power from wind. MAGLEV is short for "magnetically levitated", meaning the design incorporates magnets to "float" or suspend system components. Therefore, in this paper, an advanced level vertical wind turbine using MAGLEV mechanism is designed and implemented. In this technology, a VAWT, neodymium magnets, black magnets which are attached with wooden disk. Power is generated with an axial flux generator, which incorporates the use of permanent magnets and a set of coils. This designed MAGLEV wind turbine is independent of wind direction. Also, it can operate under low wind speed condition. | |