|  |  |  |  |
| --- | --- | --- | --- |
| **Title:** | Thyristor-based Rechargeable Battery Charger | | |
| **Author(s) Name:** | Sheikh, Protik & Riyad, Tarifuzzaman & Dey, Bezon & Alam, Sadman & Shufian, Abu & Ruddra, Istiaq | | |
| **Contact Email(s):** | protik@aiub.edu | | |
| **Published Journal Name:** | Journal of Engineering Research and Reports (JERR) | | |
| **Type of Publication:** | Journal | | |
| **Volume:** | 26 | Issue | 3 |
| **Publisher:** | Journal of Engineering Research and Reports | | |
| **Publication Date:** | 29th February 2024 | | |
| **ISSN:** | 2582-2926 | | |
| **DOI:** | https://doi.org/10.9734/jerr/2024/v26i31097 | | |
| **URL:** | https://journaljerr.com/index.php/JERR/article/view/1097 | | |
| **Other Related Info.:** | Page 104-112 | | |
|  | | | |

|  |  |
| --- | --- |
| **Abstract:** |  |
| In this project, our main objective is to design an automatic battery charger using Silicon-Controlled Rectifier (SCR) and simulate their operation. Batteries play a crucial role in safely storing electricity by converting electrical energy into chemical energy. The primary focus of our project is on thyristor-based rechargeable battery chargers, known for their high quality and competitive pricing. We delve into the design and simulation of automatic battery chargers employing SCR technology. This article encompasses the simulation, implementation, and partial construction of such a charger. The electronic circuit will be tailored to meet specific charging process requirements. | |