|  |  |  |  |
| --- | --- | --- | --- |
| **Title:** | Modeling Uncertainty in Renewable Energy Integration: A Robust Optimization Approach forGrid Study in Bangladesh | | |
| **Author(s) Name:** | Abu Hena Md. Shatil , Kazi Firoz Ahmed , Bismoy Jahan , Mohammad Tawhidul Alam , Tanbir Ibne Anowar | | |
| **Contact Email(s):** | k.firoz@aiub.edu | | |
| **Published Journal Name:** | **International Journal of Renewable Energy and Electrical Power Systems** | | |
| **Type of Publication:** | Journal | | |
| **Volume:** | 1 | Issue | 1 |
| **Publisher:** |  | | |
| **Publication Date:** | **06/05/2025** | | |
| **ISSN:** |  | | |
| **DOI:** |  | | |
| **URL:** |  | | |
| **Other Related Info.:** |  | | |
|  | | | |

|  |  |
| --- | --- |
| **Abstract:** |  |
| The integration of Renewable Energy Sources (RES) such as solar and wind into hybrid  power grids introduces significant variability and uncertainty, which can challenge grid  stability and reliability. This research investigates the application of robust optimization  techniques to manage these uncertainties in the hybrid power grid network of Bangladesh.  Using real-world solar and wind data, we model the fluctuations caused by climatic  variations and assess their impact on grid operations. The IEEE 16-bus network is  employed as the test system for this analysis. Our methodology includes data collection,  reprocessing, and the development of a robust optimization model to minimize worst-case  deviations in power supply while ensuring grid stability. The results, presented through  comprehensive graphs and tables, demonstrate the effectiveness of the proposed  approachin optimizing power dispatch, reducing costs, and enhancing reliability metrics.  Comparative analysis reveals that robust optimization outperforms traditional methods,  offering superior grid stability and cost-efficiency under uncertain conditions. This study  provides a robust framework for managing RES variability in Bangladesh’s hybrid  power grid, contributing tothe development of resilient and sustainable energy systems. | |