|  |  |  |  |
| --- | --- | --- | --- |
| **Title:** | Design and Analysis of IoT-based Remote Load Monitoring and Outage Management System | | |
| **Author(s) Name:** | Ahmed Muntasir Anwar, Md. Rifat Hazari and Mohammad Abdul Mannan | | |
| **Contact Email(s):** | rifat@aiub.edu | | |
| **Published Journal Name:** | AIUB Journal of Science and Engineering (AJSE) | | |
| **Type of Publication:** | Journal | | |
| **Volume:** | 22 | Issue | 1 |
| **Publisher:** | American International University-Bangladesh (AIUB) | | |
| **Publication Date:** | May 9, 2023 | | |
| **ISSN:** | 1608 – 3679 | | |
| **DOI:** | https://doi.org/10.53799/ajse.v22i1.552 | | |
| **URL:** | https://ajse.aiub.edu/index.php/ajse/article/view/552 | | |
| **Other Related Info.:** | Page 94-104 | | |
|  | | | |

|  |  |
| --- | --- |
| **Abstract:** |  |
| An essential instrument for the operation of a power system is to monitor and analyze the data to find the fault and rectify it before the system collapses completely. This paper intents to utilize the idea to create a control system that will fulfill objectives like monitoring vital parameters controlling the power distribution, outage management by fault detection based on the variation of Voltage, Frequency, and Current & protection of the Circuit against any significant incidents by isolating the load from utility and flagging the information through feedback to the utility authority. The Project implements the high-end technology for IoT applications that will connect with the Microcontroller to receive the data at regular intervals and post the timestamped data in a cloud platform for remote monitoring and archiving. This innovation can reduce human dependency and overcome the whole outage situation by building a two-way communication that means electricity and information are traded between consumers and utilities to capitalize on the efficiency of a grid system. The proposed model offers intelligent monitoring of the timestamped data with remote access & historical data archiving for a better load profile. An outage management system is designed for the proposed system by intellectual fault detection through Voltage, Frequency & current variation, and isolation of the faulty part from the entire system, maintaining an auto circuit recloser application before the permanent isolation for reducing the human interaction & flagging the outage information & supply emergency backup during the shutdown period, and in the process, helping the power grid from total power outage or blackout. | |